EMS New Electric Gate

In season the old outer gates will be secured in the open position

To open the gate phone 07849 357188 from a registered mobile phone

or

at the keypad enter 230980⏎ to open the gate fully

at the keypad enter 120883⏎ to open the gate 1 meter (pedestrian)

The gate has now been reprogrammed to close 5 seconds after the photocell beam has been interrupted then re-made (drive through) there is, therefore, no need to do anything to close the gate, it will close itself

Please do not tailgate anyone in front of you who has already opened the gate, if the gate is closing when you approach, tell it to open again with a phone call or code at the keypad

It is very important that you stay at the gate until it has fully closed into its dock especially in windy conditions, if the wind causes the gate to miss its dock an emergency stop will be initiated and you must then re-open the gate and let it close again into its dock

In winter the old outer gates will be locked shut and the new electric gate will operate as it does in season, so, if you come to the club out of season you will first need to open the old outer gates fully outwards and secure them in the open position, then operate the electric gate as normal, when leaving secure the old outer gates in the closed position and lock them. IN THIS SITUATION IT IS IMPERATIVE THAT YOU SECURE THE GATES IN THE OPEN POSITION SO THAT ANY WIND CAN NOT CLOSE THE OPEN GATES, IF THIS HAPPENS THE NEW ELECTRIC GATE WILL BE SEVERELY DAMAGED